From c53fbc24e989857289cceeed2a88477aeabe0158 Mon Sep 17 00:00:00 2001
From: Andrew Guschin <saintruler@gmail.com>
Date: Sat, 2 Oct 2021 22:02:39 +0400
Subject: =?UTF-8?q?=D0=9F=D0=BE=D0=BF=D1=80=D0=B0=D0=B2=D0=B8=D0=BB=20?=
 =?UTF-8?q?=D0=BE=D1=82=D1=81=D1=82=D1=83=D0=BF=D1=8B=20=D0=B2=20=D0=BB?=
 =?UTF-8?q?=D0=B5=D0=BA=D1=86=D0=B8=D0=B8=20=D0=BF=D0=BE=20=D0=9A=D0=BE?=
 =?UTF-8?q?=D0=BC=D0=BF=D1=8C=D1=8E=D1=82=D0=B5=D1=80=D0=BD=D1=8B=D0=BC=20?=
 =?UTF-8?q?=D1=81=D0=B5=D1=82=D1=8F=D0=BC?=
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

---
 sem5/computer-networks/lectures/lecture5.tex | 10 +++++-----
 1 file changed, 5 insertions(+), 5 deletions(-)

(limited to 'sem5/computer-networks/lectures/lecture5.tex')

diff --git a/sem5/computer-networks/lectures/lecture5.tex b/sem5/computer-networks/lectures/lecture5.tex
index f09cea0..13cf56b 100644
--- a/sem5/computer-networks/lectures/lecture5.tex
+++ b/sem5/computer-networks/lectures/lecture5.tex
@@ -8,8 +8,8 @@ Ethernet.
 
 Существует два варианта технологии Ethernet:
 \begin{itemize}
-    \item Ethernet на разделяемой среде;
-    \item Коммутируемый вариант Ethernet.
+  \item Ethernet на разделяемой среде;
+  \item Коммутируемый вариант Ethernet.
 \end{itemize}
 
 В первом случае все узлы разделяют общую среду передачи данных. То есть 
@@ -19,9 +19,9 @@ Ethernet.
 
 Каналы связи бывают трёх типов:
 \begin{itemize}
-    \item Симплексные;
-    \item Полудуплексные;
-    \item Полнодуплексные.
+  \item Симплексные;
+  \item Полудуплексные;
+  \item Полнодуплексные.
 \end{itemize}
 
 2. Когда сеть Ethernet не использует разделяемую среду, а строится на коммутаторах,
-- 
cgit v1.2.3

